version 15.6
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R6
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
no ip icmp rate-limit unreachable
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
redundancy
!
no cdp log mismatch duplex
!
ip tcp synwait-time 5
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 192.0.2.6 255.255.255.255
 ipv6 address 2001:DB8::6/128
!
interface Ethernet0/0
 description TO R5 (PE)
 ip address 10.5.6.6 255.255.255.0
 ipv6 address FE80::6 link-local
 ipv6 address FC00:10:5:6::6/64
!
interface Ethernet0/1
 description TO R4 (PE)
 ip address 10.4.6.6 255.255.255.0
 ipv6 address FE80::6 link-local
 ipv6 address FC00:10:4:6::6/64
!
interface Ethernet0/2
 no ip address
!
interface Ethernet0/3
 no ip address
!
router bgp 65006
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor 10.4.6.4 remote-as 65000
 neighbor 10.5.6.5 remote-as 65000
 neighbor FC00:10:4:6::4 remote-as 65000
 neighbor FC00:10:5:6::5 remote-as 65000
 !
 address-family ipv4
  network 192.0.2.6 mask 255.255.255.255
  neighbor 10.4.6.4 activate
  neighbor 10.5.6.5 activate
  maximum-paths 2
 exit-address-family
 !
 address-family ipv6
  maximum-paths 2
  network 2001:DB8::6/128
  neighbor FC00:10:4:6::4 activate
  neighbor FC00:10:5:6::5 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip ssh server algorithm encryption aes128-ctr aes192-ctr aes256-ctr
ip ssh client algorithm encryption aes128-ctr aes192-ctr aes256-ctr
!
ipv6 ioam timestamp
!
!
!
control-plane
!
!
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 privilege level 15
 logging synchronous
line aux 0
 exec-timeout 0 0
 privilege level 15
 logging synchronous
line vty 0 4
 login
 transport input none
!
!
end